**HotTab Release Notes**

|  |
| --- |
| **PRODUCT: Handheld Algiz 10x** |

|  |  |  |
| --- | --- | --- |
| **Software Version** | | **HotTab\_40.2.31** |
| **DATE:** | | 05/28/2021 |
| **CHANGE REASON:**  1-Bug Fixed 2- Function Added | | |
| **New Features:** |  | |
| **Fixed Bugs** | * Fixed battery level is displaying an abnormal percentage. | |
| **Know Errata/**  **Limitations** |  | |

|  |  |  |
| --- | --- | --- |
| **Software Version** | | **HotTab\_40.2.30** |
| **DATE:** | | 02/25/2019 |
| **CHANGE REASON:**  1-Bug Fixed 2- Function Added | | |
| **New Features:** |  | |
| **Fixed Bugs** | * Remove device OSK-Correction(touchkeyboard) | |
| **Know Errata/**  **Limitations** |  | |

|  |  |  |
| --- | --- | --- |
| **Software Version** | | **HotTab\_40.2.29** |
| **DATE:** | | 07/09/2018 |
| **CHANGE REASON:**  1-Bug Fixed 2- Function Added | | |
| **New Features:** | * Add device OSK-Correction(touchkeyboard) for windows 10 version 1709 or later.(For A10XV2) | |
| **Fixed Bugs** |  | |
| **Know Errata/**  **Limitations** |  | |

|  |  |  |
| --- | --- | --- |
| **Software Version** | | **HotTab\_40.2.28** |
| **DATE:** | | 03/02/2018 |
| **CHANGE REASON:**  1-Bug Fixed 2- Function Added | | |
| **New Features:** | * Handheld requires change backup battery display behavior.   LOW = Ship mode or 0-70% charge  HIGH = 70-100% charge | |
| **Fixed Bugs** |  | |
| **Know Errata/**  **Limitations** |  | |

|  |  |  |
| --- | --- | --- |
| **Software Version** | | **HotTab\_40.2.27** |
| **DATE:** | | 02/13/2018 |
| **CHANGE REASON:**  1-Bug Fixed 2- Function Added | | |
| **New Features:** |  | |
| **Fixed Bugs** | * Modify the backup battery does not exist show empty and does not blink. | |
| **Know Errata/**  **Limitations** |  | |

|  |  |  |
| --- | --- | --- |
| **Software Version** | | **HotTab\_40.2.26** |
| **DATE:** | | 01/25/2018 |
| **CHANGE REASON:**  1-Bug Fixed 2- Function Added | | |
| **New Features:** | * Add device OSK-Correction(touchkeyboard) for windows 10 version 1709(A10XV2) | |
| **Fixed Bugs** |  | |
| **Know Errata/**  **Limitations** |  | |

|  |  |  |
| --- | --- | --- |
| **Software Version** | | **HotTab\_40.2.25** |
| **DATE:** | | 08/15/2017 |
| **CHANGE REASON:**  1-Bug Fixed 2- Function Added | | |
| **New Features:** |  | |
| **Fixed Bugs** | * Fixed main page Touch Modes icon sometimes fail in windows7 (A10XV3) | |
| **Know Errata/**  **Limitations** |  | |

|  |  |  |
| --- | --- | --- |
| **Software Version** | | **HotTab\_40.2.24** |
| **DATE:** | | 08/01/2017 |
| **CHANGE REASON:**  1-Bug Fixed 2- Function Added | | |
| **New Features:** | * Modify token " UserPermissionLock" in HottabCfg.ini , "UserPermissionLock =0" is unlock all user permission funciton, "UserPermissionLock =1" is lock all user permission funciton, | |
| **Fixed Bugs** |  | |
| **Know Errata/**  **Limitations** |  | |

|  |  |  |
| --- | --- | --- |
| **Software Version** | | **HotTab\_40.2.23** |
| **DATE:** | | 07/14/2017 |
| **CHANGE REASON:**  1-Bug Fixed 2- Function Added | | |
| **New Features:** | * Add token " UserPermissionLock" in HottabCfg.ini , "UserPermissionLock =0" is unlock user permission funciton, "UserPermissionLock =1" is lock user permission funciton, | |
| **Fixed Bugs** |  | |
| **Know Errata/**  **Limitations** |  | |

|  |  |  |
| --- | --- | --- |
| **Software Version** | | **HotTab\_40.2.22** |
| **DATE:** | | 05/18/2017 |
| **CHANGE REASON:**  1-Bug Fixed 2- Function Added | | |
| **New Features:** | * Add user permission limit device and function key settings can not be used. * Update the new installer. | |
| **Fixed Bugs** |  | |
| **Know Errata/**  **Limitations** |  | |

|  |  |  |
| --- | --- | --- |
| **Software Version** | | **HotTab\_A40.2.21** |
| **DATE:** | | 04/27/2017 |
| **CHANGE REASON:**  1-Bug Fixed 2- Function Added | | |
| **New Features:** |  | |
| **Fixed Bugs** | * Fixed F2 charm bar(home + C) not work in windows 8.1. | |
| **Know Errata/**  **Limitations** |  | |

|  |  |  |
| --- | --- | --- |
| **Software Version** | | **HotTab\_A40.2.20** |
| **DATE:** | | 04/24/2017 |
| **CHANGE REASON:**  1-Bug Fixed 2- Function Added | | |
| **New Features:** |  | |
| **Fixed Bugs** | * Modify backup battery status switch default on show backup battery information. | |
| **Know Errata/**  **Limitations** | **HotTab\_A40.2.10** charm bar(home + C) at Win8 | |

|  |  |  |
| --- | --- | --- |
| **Software Version** | | **HotTab\_A40.2.20** |
| **DATE:** | | 03/15/2017 |
| **CHANGE REASON:**  1-Bug Fixed 2- Function Added | | |
| **New Features:** | * Add Model Name in BIOS ver, EC Ver, HotTab Ver, OS Ver. | |
| **Fixed Bugs** |  | |
| **Know Errata/**  **Limitations** | **HotTab\_A40.2.10** charm bar(home + C) at Win8 | |

|  |  |  |
| --- | --- | --- |
| **Software Version** | | **HotTab\_A40.2.19** |
| **DATE:** | | 11/10/2016 |
| **CHANGE REASON:**  1-Bug Fixed 2- Function Added | | |
| **New Features:** |  | |
| **Fixed Bugs** | * Fix Touch Modes Control UI position error in windows 7 system. | |
| **Know Errata/**  **Limitations** | **HotTab\_A40.2.10** charm bar(home + C) at Win8 | |

|  |  |  |
| --- | --- | --- |
| **Software Version** | | **HotTab\_A40.2.18** |
| **DATE:** | | 11/01/2016 |
| **CHANGE REASON:**  1-Bug Fixed 2- Function Added | | |
| **New Features:** | * Add backup battery status swtich in hottab setting page. Default switch off hide backup battery information. | |
| **Fixed Bugs** |  | |
| **Know Errata/**  **Limitations** | **HotTab\_A40.2.10** charm bar(home + C) at Win8 | |

|  |  |  |
| --- | --- | --- |
| **Software Version** | | **HotTab\_A40.2.17** |
| **DATE:** | | 10/03/2016 |
| **CHANGE REASON:**  1-Bug Fixed 2- Function Added | | |
| **New Features:** | * For SAAB project, delete backup battery information. | |
| **Fixed Bugs** |  | |
| **Know Errata/**  **Limitations** | **HotTab\_A40.2.10** charm bar(home + C) at Win8 | |

|  |  |  |
| --- | --- | --- |
| **Software Version** | | **HotTab\_A40.2.16** |
| **DATE:** | | 09/13/2016 |
| **CHANGE REASON:**  1-Bug Fixed 2- Function Added | | |
| **New Features:** | * New Touch Modes Control:   - Pressing "lock" should show Current Touch Mode  - Once inside "touch changing mode" unit should Toggle between touch modes when "lock" is pressed. (support Normal Mode, Rain Mode, Glove Mode, Touch Locked)  - After leaving the unit at Mode. Icon shall be visable for 5 seconds.  - If unit is left in "Touch Locked" icon shall be present for 5 seconds. After 5 seconds th icon shall still be present but in a smaller version at the lower end of the screen. Icon is present as long as the touch is locked.  - Currently there is delay to get out of "touch locked". I have to hold the down the lock key to get out of locked touch. Please remove this delay. | |
| **Fixed Bugs** |  | |
| **Know Errata/**  **Limitations** | **HotTab\_A40.2.10** charm bar(home + C) at Win8 | |

|  |  |  |
| --- | --- | --- |
| **Software Version** | | **HotTab\_A40.2.15** |
| **DATE:** | | 08/29/2016 |
| **CHANGE REASON:**  1-Bug Fixed 2- Function Added | | |
| **New Features:** | * Remove touch lock from the menu. * Move Touch Set to menu.(The same behavior with lock key) * The physical "Lock key" should change between touch modes when pressed. Unlock touch lock long press "Lock key".   (1)Normal mode  (2)Rain mode  (3)Glove mode  (4)Touch lock | |
| **Fixed Bugs** |  | |
| **Know Errata/**  **Limitations** | **HotTab\_A40.2.10** charm bar(home + C) at Win8 | |

|  |  |  |
| --- | --- | --- |
| **Software Version** | | **HotTab\_A40.2.14** |
| **DATE:** | | 08/02/2016 |
| **CHANGE REASON:**  1-Bug Fixed 2- Function Added | | |
| **New Features:** | * Suppourt MB-1XX and MB-2XX F3 function key different behavior.   (1)MB-1XX: F3 Key is Home key.  (2)MB-2XX: F3 Key is touch lock key. | |
| **Fixed Bugs** |  | |
| **Know Errata/**  **Limitations** | **HotTab\_A40.2.10** charm bar(home + C) at Win8 | |

|  |  |  |
| --- | --- | --- |
| **Software Version** | | **HotTab\_A40.2.13** |
| **DATE:** | | 07/05/2016 |
| **CHANGE REASON:**  1-Bug Fixed 2- Function Added | | |
| **New Features:** | * When backup battery use only(AC annd Main Battery not exist). Switch brightness to minimum and CPU processer to 50%. * Modify backup battery capacity >= 80% is high level. | |
| **Fixed Bugs** | N/A | |
| **Know Errata/**  **Limitations** | **HotTab\_A40.2.10** charm bar(home + C) at Win8 | |

|  |  |  |
| --- | --- | --- |
| **Software Version** | | **HotTab\_A40.2.12** |
| **DATE:** | | 06/07/2016 |
| **CHANGE REASON:**  1-Bug Fixed 2- Function Added | | |
| **New Features:** | * Add touch three mode support. * Add small battery warning "Need Replacement" and modify battery low icon. * Removed F3 key , add touch lock key | |
| **Fixed Bugs** | N/A | |
| **Know Errata/**  **Limitations** | **HotTab\_A40.2.10** charm bar(home + C) at Win8 | |

|  |  |  |
| --- | --- | --- |
| **Software Version** | | **HotTab\_A40.2.11** |
| **DATE:** | | 09/17/2015 |
| **CHANGE REASON:**  1-Bug Fixed 2- Function Added | | |
| **New Features:** | N/A | |
| **Fixed Bugs** | * Change F2 support Action center(home + A) at Win10 | |
| **Know Errata/**  **Limitations** | **HotTab\_A40.2.10** charm bar(home + C) at Win8 | |

|  |  |  |
| --- | --- | --- |
| **Software Version** | | **HotTab\_A40.2.10** |
| **DATE:** | | 06/22/2015 |
| **CHANGE REASON:**  1-Bug Fixed 2- Function Added | | |
| **New Features:** | N/A | |
| **Fixed Bugs** | * Fixed HotTab menu new lock function, press the menu button a couple of times after locking the screen you get access to the toolbar * Fixed Menu function fails after resume from suspend and Touch Un-locked | |
| **Know Errata/**  **Limitations** |  | |

|  |  |  |
| --- | --- | --- |
| **Software Version** | | **HotTab\_A40.2.09** |
| **DATE:** | | 06/12/2015 |
| **CHANGE REASON:**  1-Bug Fixed 2- Function Added | | |
| **New Features:** | N/A | |
| **Fixed Bugs** | * At HotTab menu new lock function, to aviod charm bar shows, lock area includes OSD function key | |
| **Know Errata/**  **Limitations** | To fixed charm bar, it needs to click rear form that does not use function call | |

|  |  |  |
| --- | --- | --- |
| **Software Version** | | **HotTab\_A40.2.08 (reserve)** |
| **DATE:** | | 04/27/2015 |
| **CHANGE REASON:**  1-Bug Fixed 2- Function Added | | |
| **New Features:** | N/A | |
| **Fixed Bugs** | * restore GPS setting during hotTab loading | |
| **Know Errata/**  **Limitations** |  | |

|  |  |  |
| --- | --- | --- |
| **Software Version** | | **HotTab\_A40.2.07** |
| **DATE:** | | 03/19/2015 |
| **CHANGE REASON:**  1-Bug Fixed 2- Function Added | | |
| **New Features:** | N/A | |
| **Fixed Bugs** | * fixed camera ap flsh control panel will auto show after resume from picture preview mode. | |
| **Know Errata/**  **Limitations** |  | |

|  |  |  |
| --- | --- | --- |
| **Software Version** | | **HotTab\_A40.2.05** |
| **DATE:** | | 12/27/2014 |
| **CHANGE REASON:**  1-Bug Fixed 2- Function Added | | |
| **New Features:** | N/A | |
| **Fixed Bugs** | * Fixed when press OSK’s or real keyboard’s arrow key and enter key will send double time. * Fixed when enable then disable AutoBrightness, next time adjust brightness sometimes that value will not correct. because auto brightness enable that does not keep value after adjustement. | |
| **Know Errata/**  **Limitations** |  | |

|  |  |  |
| --- | --- | --- |
| **Software Version** | | **HotTab\_A40.2.04** |
| **DATE:** | | 12/09/2014 |
| **CHANGE REASON:**  1-Bug Fixed 2- Function Added | | |
| **New Features:** | N/A | |
| **Fixed Bugs** | * New Brightness/Volume UI | |
| **Know Errata/**  **Limitations** | Base on resistive touch, scorll bar can not adjust value smoothly. User needs use arrows key. | |

|  |  |  |
| --- | --- | --- |
| **Software Version** | | **HotTab\_A40.2.03** |
| **DATE:** | | 12/02/2014 |
| **CHANGE REASON:**  1-Bug Fixed 2- Function Added | | |
| **New Features:** | N/A | |
| **Fixed Bugs** | * Brightness and Volume is OK under settings. But the graphics must be adjusted to match hottab (or default Win8 volume/brightness UI) * Brightness and Volume (when chosen in hottab) must be adjustable with arrow keys. * Auto brightness on/off must be available like before when Brightness is visible. * Devices - remove Light Sensor (see previous above) - Rename GPS Antennas to "External GPS" - Rename WWAN Antenna to "External WWAN" - Place both External GPS and External WWAN on the left side (where GPS Antenna and light Sensor is now placed) | |
| **Know Errata/**  **Limitations** | N/A | |

|  |  |  |
| --- | --- | --- |
| **Software Version** | | **HotTab\_A40.2.02** |
| **DATE:** | | 11/26/2014 |
| **CHANGE REASON:**  1-Bug Fixed 2- Function Added | | |
| **New Features:** | N/A | |
| **Fixed Bugs** | * Enter S3 close camera form to fix issue ”HotTab camera UI,flash icon keeps ON after resume from suspend if flash ON first” * Reduce show battery info time to 3 seconds to fix issue”Battery information update needs 15 secs if restore” * Disable chargeTime string to fix issue”HotTab would shows "BAT2ChargeTime" during BackUp battery discharge” * Modify UI to fix issue ” "Function 3" short press UI does NOT same as "Fuction 1"/"Function 2" | |
| **Know Errata/**  **Limitations** | N/A | |

|  |  |  |
| --- | --- | --- |
| **Software Version** | | **HotTab\_A40.2.01** |
| **DATE:** | | 11/17/2014 |
| **CHANGE REASON:**  1-Bug Fixed 2- Function Added | | |
| **New Features:** | N/A | |
| **Fixed Bugs** | * First Version * Four page: rotation, camera, device, setting | |
| **Know Errata/**  **Limitations** | N/A | |